**Scale Button Adjustment Steps**  
The purpose of this canvas to to provide a step by step guide for installing the scale button correctly.

* Procedure Steps
* Video Tutorial

Procedure:

1. Checking Alignment:
   1. Make sure the rectangular portion on the scale button lines up with the rectangular portion on the scale as depicted below:
2. Placing The Button:
   1. Using 2 fingers, place the scale button on the scale as on the scale in the orientation shown above. Do not press too hard on the scale.
3. Verifying Install:
   1. If properly done it should look like the image below.
   2. Button should be flat and snapped into place. A little bit of wiggle is normal but it shouldn't pull or fall off easily.
4. Calibrate Scales:
   1. It is important to remember to recalibrate the scales after any change to the scale button.

Video:

Watch this instructional video for more detailed steps. <https://acceleranthq.slack.com/files/U0724UAR2D8/F07CW02P76W/img_5226.mov>